Snap Hooks/Carabiners Annual Inspection

|  |
| --- |
| Hook/Carabiner Mfr./Model/Name  |
| Serial Number  | Lot Number  |
| Date of Manufacture Click to enter date | Date of Purchase Click to enter date |
| Inspected By (Competent Person)  | Date Inspected Click to enter date |

|  |  |  |  |
| --- | --- | --- | --- |
| **Components** | **Pass** | **Fail** | **Comments** |
| **Physical Damage** |
| 1 | Inspect for cracks, sharp edges, burrs, deformities and proper locking operations  |[ ] [ ]    |
| 2 | Other:  |[ ] [ ]    |
| **Excessive Corrosion** | **Pass** | **Fail** |  |
| 3 | Inspect for corrosion, which affects the operation and/or strength |[ ] [ ]    |
| 4 | Other:  |[ ] [ ]    |
|  **Markings** | **Pass** | **Fail** |  |
| 5 | Inspect and make certain marking(s) are legible |[ ] [ ]    |
| 6 | Other:  |[ ] [ ]    |
| **Other** | **Pass** | **Fail** |  |
| 7 |   |[ ] [ ]    |
| **Other**  |
| 8 |   |[ ] [ ]   |
| **Overall Assessment** | **Pass** | **Fail** |  |
|  |[ ] [ ]    |
| Comments: Click to enter text |

**If snap hook/carabiner fails, it must be tagged and taken out of service.**