Full-Body Harness Annual Inspection

|  |
| --- |
| Harness Mfr./Model/Name  |
| Serial Number  | Lot Number  |
| Date of Manufacture Click to enter date | Date of Purchase Click to enter date |
| Inspected By (Competent Person)  | Date Inspected Click to enter date |

|  |  |  |  |
| --- | --- | --- | --- |
| **Components** | **Pass** | **Fail** | **Comments** |
| **Hardware** |
| 1 | Inspect D-rings, buckles, keepers and back pads. Inspect for damage, distortion, sharp edges, burrs, cracks, and corrosion |[ ] [ ]    |
| 2 | Other:  |[ ] [ ]    |
| **Webbing** | **Pass** | **Fail** |  |
| 3 | Inspect for cuts, burns, tears, abrasions, frays, excessive soiling and discoloration |[ ] [ ]    |
| 4 | Other:  |[ ] [ ]    |
|  **Stitching** | **Pass** | **Fail** |  |
| 5 | Inspect for pulled or cut stitches |[ ] [ ]    |
| 6 | Other:  |[ ] [ ]    |
| **Labels** | **Pass** | **Fail** |  |
| 7 | Inspect, making certain all labels are securely held in place and are legible |[ ] [ ]    |
| **Other**   | **Pass** | **Fail** |  |
| 8 |   |[ ] [ ]    |
| **Overall Assessment** | **Pass** | **Fail** |  |
|  |[ ] [ ]    |
| Comments: Click to enter text |

**If harness fails, it must be tagged and taken out of service.**