Snap Hooks/Carabiners Annual Inspection

|  |  |  |
| --- | --- | --- |
| Hook/Carabiner Mfr./Model/Name | | |
| Serial Number | Lot Number | |
| Date of Manufacture Click to enter date | Date of Purchase Click to enter date | |
| Inspected By (Competent Person) | | Date Inspected Click to enter date |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Components** | | **Pass** | **Fail** | **Comments** |
| **Physical Damage** | | | | |
| 1 | Inspect for cracks, sharp edges, burrs, deformities and proper locking operations |  |  |  |
| 2 | Other: |  |  |  |
| **Excessive Corrosion** | | **Pass** | **Fail** |  |
| 3 | Inspect for corrosion, which affects the operation and/or strength |  |  |  |
| 4 | Other: |  |  |  |
| **Markings** | | **Pass** | **Fail** |  |
| 5 | Inspect and make certain marking(s) are legible |  |  |  |
| 6 | Other: |  |  |  |
| **Other** | | **Pass** | **Fail** |  |
| 7 |  |  |  |  |
| **Other** | | | | |
| 8 |  |  |  |  |
| **Overall Assessment** | | **Pass** | **Fail** |  |
|  |  |  |
| Comments: Click to enter text | | | | |

**If snap hook/carabiner fails, it must be tagged and taken out of service.**